Northern Illinois University

*NIU Construction Standards*

*Division 08 1416 – Flush Wood Doors*

March 2014, Rev 00











Book match veneers on double doors.

Wood doors to be solid core 1-3/4" thick with veneer min. 1/50" thick. Veneer for doors with transparent finishes shall be Red Oak – Plain Sliced. Transparent finish doors are to be factory finished, with satin sheen.

Provide blocking for all necessary hardwood blocking for closer, lock, and hinges.

Flush Wood Doors Div 08 1416 Page **1** of **1**