

*NIU Design and Construction Standards*

*Division 22 1116 – Domestic Water Piping*

February 2015, Draft 00

**22 1116 – Domestic Water Piping**

PART 1. - GENERAL

Domestic Water Inside Supply Pipe







2.5” or less - Type L copper. No-lead solder or grooved fittings.

3” or more - Ordinary duty weight galvanized steel. Flanged or grooved fittings. Stainless steel ball Isolation valves on all branches off domestic mains.

**This section of the NIU Design Requirements establishes minimum requirements only.**

**It should not be used as a complete specification.**

Domestic Water Piping Div 22 1116 Page 1 of 1